Specification:

1.Effective measurement range:

Binocular pupillary distance: 45～82 mm

Left or right pupillary distance: 22.5～41 mm

2.Step: ∞, 2m, 1m, 65cm, 50cm, 40cm,35cm,30cm

3.Indication error：≤0.5mm

4. Asymmetrical error: ≤0.5mm

5.Rounding error：≤0.5mm

6.Distance of target：30 cm ～∞

7.Power source：5# AA battery/2\*1.5V

8.Size and weight: 221mm(L)×166mm(W)×63mm(H) 0.64kg